[Information]
; (Latest Translator, First Translator, Second Translator ...)
TRANSLATOR=ICM
VERSION=2.7.0

[Language]
LANGUAGE=Azeri
CHARACTER_CODE=Unicode (UTF-16, LE, w/ BOM)
LOCALE_ID=0x042C, 0x082C

[Url]
WIKIPEDIA_SMART=https://en.wikipedia.org/wiki/Self-Monitoring%2C_Analysis_and_Reporting_Technology

[Menu]
FILE=&Fayl
CUSTOMIZE=&Nizamlamaq
EXIT=&Çıxış
EDIT=&Düzəliş
COPY=&Köçürtmək
FUNCTION=&Funksiya
HIDE_SMART_INFO= &S.M.A.R.T. informasiyanı gizlətmək
HIDE_SERIAL_NUMBER=Seriya nömrəsini gizlətmək &
SHOW_DRIVE_LETTER=Hissənin həriflərini göstərmək&
ADVANCED_DISK_SEARCH=&Disklərin geniş axtarışı
EVENT_LOG=&Hadisələrin qeydiyatı
AAM_APM_CONTROL=İdarə etmə AA&M/APM
AUTO_AAM_APM_ADAPTION=Avtonizamlama AAM/A&PM
RESIDENT=&Agentin işə salınması
STARTUP=&Avto işə salma
OPEN_DISK_MANAGEMENT= "&Disk menecerinin" işə salınması
OPEN_DEVICE_MANAGER= "&Qurğular növbətçisinin" işə salınması
ADVANCED_FEATURE=Geniş &nizamlamalar
REFRESH=&yenilə
RESCAN=yenidən&işəs salma
DISABLE=&söndürmək
AUTO_REFRESH=&Avtoyeniləmə
AUTO_REFRESH_TARGET=seçilənin avto yenilənməsi&
AUTO_REFRESH_TARGET_ALL_DISK=avtoyeniləmə -ütün diskləri seçmək
AUTO_REFRESH_UNTARGET_ALL_DISK=avtoyeniləmə - bütün disklərdən seçimi ləğv etmək
WAIT_TIME_AT_STARTUP=&işə salmanı dayandırmaq
GRAPH=&Qrafik
THEME=&Mövzu
DISK=&Disk
HELP=&Məlumat
HELP_WEB=&Məlumat [Web]
HELP_ABOUT=& CrystalDiskInfo proqramı haqqında
HELP_ABOUT_SMART= &S.M.A.R.T. (Wikipedia) [Web] texnalogiyası haqqında
LANGUAGE=&Dil
ITEM=&Bənd
TEMPERATURE_TYPE=&Temperatur kəmiyyəti
CELSIUS=Selsi (°C)
FAHRENHEIT=Farinqeyt (°F)
HEALTH_STATUS_SETTING=& Тех. vəziyyətin nizamlanması

;Graph
OPTION=&Nizamlamalar
LEGEND_POSITION=&Əfsanənin yeri
NORTH_WEST=&Şimali-qərb
NORTH_EAST=Şimali-şərq
SOUTH_WEST=Cənubi-qərb
SOUTH_EAST=&Cənubi-şərq
MAX_PLOT_POINT=&Düzülüşün maksimal nöqtəsi
TIME_FORMAT=&Vaxtın formatı
PAINT_WEEKEND=&Boş vaxtları göstərmək
ALL=&Bütün

;2.7.0
COPY_OPTION=Parametrlərin &kopyalanması
RESIDENT_STYLE=Yerli  üs&lub
MINIMIZE=Bağlamaq
HIDE=Gizlətmək

;3.0.0
ZOOM=&Zoom
AUTO=&Auto
ATTRIBUTE=&Attribute

;3.5.0
ASCII_VIEW=ASCII View
AUTO_DTECTION=Auto Detection
SECOND=san.
MINUTE=dəq.
HOUR=hour

:3.9.4
WORKAROUND=W&orkaround

;4.0.0
ALERT_MAIL=Alert Mail
MAIL_SETTINGS=Mail Settings
SMART_IN_ENGLISH=S.M.A.R.T. in English
FONT_SETTING=Font Setting

;5.0.0
ALERT_FEATURES=A&lert Features
ALARM_HISTORY=Alarm History
ALERT_SOUND=Alert Sound
SOUND_SETTINGS=Sound Settings
GADGET_SUPPORT=Gadget Support
INSTALL_GADGET=Install Gadget
ENABLE_AUTO=Enable (Auto Detection)
ENABLE_ALL=Enable (All Disks)
ENABLE_RAID=Enable (RAID Volume Only)

;6.0.0
HIDE_NO_SMART_DISK=&Hide No S.M.A.R.T. Disk
GREEN_MODE=&Green Mode

;8.6.0
SAVE_TEXT=Save (&text)
SAVE_IMAGE=&Save (image)

[TrayMenu]
EXIT=Çıxış
REFRESH=Yeniləmək
RESIDENT=Agentin işə salınması
ENABLE=Yandırmaq
DISABLE=Sönülü
ENABLE_ALL=Hər seyi yandırmaq
DISABLE_ALL=Hər şeyi söndürmək
AUTO_REFRESH=Avtoyeniləmə
AUTO_REFRESH_TARGET=Seçilmişin avtoyeniləməsi
AUTO_REFRESH_TARGET_ALL_DISK=Avtoyeniləmə - bütün diskləri seçmək
AUTO_REFRESH_UNTARGET_ALL_DISK=Avto yeniləmə -Bütün disklərdən seçimi götürmək
ALARM_SETTING_TEMPERATURE=Həyacan - Temperatura
ALARM_SETTING_HEALTH_STATUS=Həyacan – Tex. vəziyyət
SHOW_MAIN_WINDOW=Əsas pəncərəni göstərmək
SHOW_TEMPERATURE_ICON=Temperaturu göstərmək
SHOW_ALL_TEMPERATURE_ICON=Bütün temperaturu göstərmək
HIDE_ALL_TEMPERATURE_ICON=Btün temperaturu gizlətmək
COLLECTIVE_SETTING=Ümumi nizamlamalar
GRAPH=Qrafik
;Added 3.0
SHOW_TEMPERATURE_ICON_ONLY=Show Temperature Icon Only

[DiskStatus]
GOOD=Yaxşı
CAUTION=Diqqət!
BAD=Pis
UNKNOWN=Naməlum
DISK=Disk

[Dialog]
LIST_ID=ID
LIST_CURRENT=Hazırki
LIST_WORST=Pis
LIST_THRESHOLD=Kandar
LIST_RAW_VALUES=Naməlum kəmiyyət
;LIST_DESCRIPTION=Təsvir
LIST_ATTRIBUTE_NAME=Atributun adı

FIRMWARE=Proqramlaşdırılan avadanlığın növü
SERIAL_NUMBER=Seria nömrəsi
INTERFACE=İnterfeys
STANDARD=Standart
TRANSFER_MODE=Məlumatların ötürmə görünüşü
BUFFER_SIZE=Buferin həcmi
NV_CACHE_SIZE= NV-keşin həcmi
ROTATION_RATE=Fırlanma sürəti
TEMPERATURE=Temperatur
POWER_ON_HOURS=Ümumi iş vaxtı
POWER_ON_COUNT=Yandırma sayı
DRIVE_LETTER=Bənddə hərif
FEATURE=Nizamlamalar
HEALTH_STATUS=Tex. vəziyyət

UNKNOWN=Неизвестно
POWER_ON_COUNT_UNIT=раз  
POWER_ON_HOURS_UNIT=saat
POWER_ON_DAYS_UNIT=gün
POWER_ON_YEARS_UNIT=il

;4.3
TOTAL_HOST_WRITES=Total Host Writes
TOTAL_HOST_READS=Total Host Reads
TOTAL_NAND_WRITES=Total NAND Writes

;4.5
WEAR_LEVELING_COUNT=Wear Leveling Count

;6.1
CURRENT_MODE_SUPPORTED_MODE=Current Mode | Supported Mode
MAJOR_VERSION_MINOR_VERSION=Major Version | Minor Version

;8.5.0
FONT_FACE=Font Face
FONT_SCALE=Font Scale (%)
DEFAULT=Default

;8.9.0
ENABLED=Enabled
DISABLED=Disabled

[Message]
DETECT_UNIT_POWER_ON_HOURS=Sərt diskin parametrləri
DETECT_DISK=Diski müəyyən etmək
PLEASE_ENABLE_WMI= WMI(Windows Management Instrumentation) işə salınması
PLEASE_RESTART_THIS_APPLICATION=Mövzunu dəyişmək üçün proqramı yenidən işə salmaq
DISK_NOT_FOUND=Disk tapılmayıb

[Alarm]
ALARM_TEMPERATURE=Həyacan - Temperatur
ALARM_HEALTH_STATUS=Həyacan – Tex. vəziyyət
DEGRADATION=Kiçiltmə
RECOVERY=Bərpa etmə
;3.5.0
INFO_HEALTH_STATUS=Info - Health Status

[Graph]
PLEASE_SELECT_ITEM=Bəndi seçin
ACTUAL_VALUE=Faktiki dəyər (Naməlum kəmiyyət)
NORMALIZED_VALUE=Nömrələnmiş dəyər (Hazırkı dəyər)
ALL_ON=Həmişə işlək
ALL_OFF=Həmişə sönük
RESET=Təkrar yığım

[Customize]
LINE_COLOR=Xətin rəngi
BACKGROUND_IMAGE=Fon
SUPPORTED_IMAGE_FORMAT=Dəstəklənən görüntü
ALL_FILES=Bütün fayllar

;5.0.0
SUPPORTED_SOUND_FORMAT=Supported Sound Format

[AamApm]
AAM_LOW=<- Sakit (80h)
AAM_HIGH=Məhsuldar (FEh) ->
AAM_RECOMMEND=Tövsiyyə olunan
APM_LOW=<- Qənaətli(01h)
APM_HIGH=Məhsuldar (FEh) ->
;3.5.0
AUTOMATIC_ACOUSTIC_MANAGEMENT=Automatic Acoustic Management (AAM)
ADVANCED_POWER_MANAGEMENT=Advanced Power Management (APM)

[WindowTitle]
ABOUT= CrystalDiskInfo proqramı haqda
GRAPH=Qrafik
CUSTOMIZE=Nizamlamaq
VERSION_INFORMATION= Versiya haqda məlumat
AAM_APM_CONTROL=AAM/APM idarə
HEALTH_STATUS_SETTING=Tex. vəziyyətin nizamlanması

;5.0.0
ALARM_HISTORY=Alarm History
SOUND_SETTINGS=Sound Settings

;5.1.0
FONT_SETTING=Font Setting

[HealthStatus]
THRESHOLD_OF_CAUTION=Diqqət Kandar
APPLY=Tədbiq etmək
DEFAULT=Tövsiyə olunan

[Smart]
UNKNOWN=Naməlum
VENDOR_SPECIFIC=Məhsuldar
01=Oxuma xətası
02=Məhsuldarlıq
03=Dövriyyə vaxtı
04=İşə salmalar/şpindelin dayanmaları
05=Yenidən qeyd olunmuş sektorlar
06=Oxuma kanalının ehtiyatı
07=Yerləşdirmə xətası
08=Axtarış vaxtı
09=İşləmə vaxtı
0A=Yenidən dövriyyə etmə cəhdləri
0B=Yenidən kalibirləşmə cəhdləri
0C=İşə salma sayı
0D=Proqram oxuma xətası
BE=Hava axının temperaturu
BF=Zərbə yüklənmələrində xəta
C0=Qidalanmanın söndürülməsində inkar
C1=Yükləmə sayları/Boşaltmalar
C2=Temperatura
C3= ECC aparatlı bərpası
C4=Əməliyyatın yenidən qeyd edilməsi
C5=Dəyişmək üçün sektorlar
C6=Sektorların düzəlməyən xətaları
C7=UltraDMA CRC-Səhvləri
C8=Yazma səhvləri
C9=Proqram yazma səhvləri
CA=Məlumatların ünvan səhvləri
CB=İşə salmada inkarlar
CC=ECC proram bərpası
CD=temperatur düşüşləri
CE=Asıllığın hündürlüyü
CF=Hazırkı hündürlük
D0=Spin Buzz
D1=Müstəqil axtarışın məhsuldarlığı
D2=Yazılmada titrəmələr
D3=Oxumada  titrəmələr
D4=yazılma vaxti titrəmə
DC=diskin yerindən oynaması
DD=Zərbədən xətalat (G-Sense)
DE=İşləmə vaxtı (saat)
DF= Yükləmə təkarları/Boşaltmalar
E0=Yüklənmə vaxtı sürtünmə gücü
E1= Yükləmə sayları/Boşaltmalar
E2=Yükləmə vaxtı
E3=Fırlanma anının gücləndirilməsi
E4=Söndürmə vaxtı düzəlişlər
E6=GMR-başlığın amplitudası
E7=Temperatura
F0=Başlığın yerdəyişmə vaxtı (saat)
FA=Oxuma vaxtı xətaların sayı

;Updated 5.4.0
F1=Total Host Writes
F2=Total Host Reads

[SmartSsd]
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
04=Start/Stop Count
05=Reallocated Sectors Count
06=Read Channel Margin
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0B=Recalibration Retries
0C=Power Cycle Count
0D=Soft Read Error Rate stab
C0=Unsafe Shutdown Count
C2=Temperature
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Uncorrectable Sector Count
; CrystalDiskInfo assign
FF=Remaining Life

;Updated 5.4.0
F1=Total Host Writes
F2=Total Host Reads

[SmartMtron]
BB=Total Erase Count

[SmartIndilinx]
01=Read Error Rate
09=Power-On Hours
0C=Power Cycle Count
B8=Initial Bad Block Count
C3=Program Failure Block Count
C4=Erase Failure Block Count
C5=Read Failure Block Count
C6=Total Count of Read Sectors
C7=Total Count of Write Sectors
C8=Total Count of Read Commands
C9=Total Count of Write Commands
CA=Total Count of Error bits from flash
CB=Total Count of Read Sectors with Correctable Bit Errors
CC=Bad Block Full Flag
CD=Maximum PE Count Specification
CE=Minimum Erase Count
CF=Maximum Erase Count
D0=Average Erase Count
D1=Remaining Drive Life

[SmartJMicron60x]
09=Power-On Hours
0C=Power Cycle Count
C2=Temperature
E5=Halt System ID, Flash ID
E8=Firmware Version Information
E9=ECC Fail Record
EA=Average Erase Count, Max Erase Count
EB=Good Block Count, System Block Count

[SmartIntel]
03=Spin Up Time
04=Start/Stop Count
05=Re-Allocated Sector Count
09=Power-On Hours Count
0C=Power Cycle Count
C0=Unsafe Shutdown Count
E1=Host Writes
E8=Available Reserved Space
E9=Media Wearout Indicator
B8=End to End Error Detection Count

;Updated 4.1
AA=Available Reserved Space
AB=Program Fail Count
AC=Erase Fail Count
BB=Uncorrectable Error Count

;Updated 4.3
AE=Unexpected Power Loss
E2=Timed Workload Media Wear
E3=Timed Workload Host Read/Write Ratio
E4=Timed Workload Timer
F1=Total LBAs Written
F2=Total LBAs Read
F9=Total NAND Writes

;Updated 5.5.0
B7=SATA Downshift Count
BE=Temperature
C7=CRC Error Count

;Updated 5.6.1
AF=Power Loss Protection Failure
C2=Temperature
C5=Pending Sector Count

;Added 6.6.0
EA=Thermal Throttle Status

[SmartSamsung]
05=Reallocated Sector Count
09=Power-on Hours
0C=Power-on Count
AF=Program Fail Count (Chip)
B0=Erase Fail Count (Chip)
B1=Wear Leveling Count
B2=Used Reserved Block Count (Chip)
B3=Used Reserved Block Count (Total)
B4=Unused Reserved Block Count (Total)
B5=Program Fail Count (Total)
B6=Erase Fail Count (Total)
B7=Runtime Bad Block (Total)
BB=Uncorrectable Error Count
BE=Airflow Temperature
C2=Temperature
C3=ECC Error Rate
C6=Off-Line Uncorrectable Error Count
C7=CRC Error Count
C9=Super cap Status
CA=SSD Mode Status
EB=POR Recovery Count
F1=Total LBA Written
F2=Total LBA Read

;Added 6.6
AA=Unused Reserved Block Count (Chip) 
AB=Program Fail Count (Chip)
AC=Erase Fail Count (Chip)
AD=Wear Leveling Count
AE=Unexpected Power Loss Count
B8=Error Detection
E9=Normalized Media Wear-out

[SmartSandForce] ;Updated (3.7.0)
01=Raw Read Error Rate
05=Retired Block Count
09=Power-on Hours
0C=Power Cycle Count
0D=Soft Read Error Rate
64=Gigabytes Erased
AA=Reserve Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B5=Program Fail Count
B6=Erase Fail Count
B8=Reported I/O Error Detection Code Errors
BB=Reported Uncorrectable Errors
C2=Temperature
C3=On-the-Fly ECC Uncorrectable Error Count
C4=Reallocation Event Count
C6=Uncorrectable Sector Count
C7=SATA R-Errors (CRC) Error Count
C9=Uncorrectable Soft Read Error Rate
CC=Soft ECC Correction Rate
E6=Life Curve Status
E7=SSD Life Left
E8=Available Reserved Space
EB=SuperCap health
F1=Lifetime Writes from Host
F2=Lifetime Reads from Host

[SmartJMicron61x] ;Added (3.9)
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0C=Power Cycle Count
A8=SATA PHY Error Count
AF=Bad Cluster Table Count (ECC Fail Count)
C0=Unexpected Power Loss Count
C2=Temperature
C5=Current Pending Sector Count
AA=Bad Block Count
AD=Erase Count

[SmartMicron] ;Added 4.0.0/ Updated 6.6.0
; RAIN = Redundant Array of Independent NAND
01=Raw Read Error Rate
05=Reallocated NAND Blocks
09=Power On Hours
0C=Power Cycle Count
0D=Soft Error Rate
0E=Device Capacity (NAND)
0F=User Capacity
10=Spare Blocks Available
11=Remaining Spare Blocks
64=Total Erase Count
AA=Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Block-Erase Count
AE=Unexpected Power Loss Count
B4=Unused Reserve NAND Blocks
B5=Unaligned Access Count
B7=SATA Interface Downshift
B8=Error Correction Count
BB=Reported Uncorrectable Errors
BC=Command Timeout Count
BD=Factory Bad Block Count
C2=Temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Smart Off-line Scan Uncorrectable Error Count
C7=Ultra DMA CRC Error Rate
CA=Percent Lifetime Used
CE=Write Error Rate
D2=Successful RAIN Recovery Count
EA=Total Bytes Read
F2=Write Protect Progress
F3=ECC Bits Corrected
F4=ECC Cumulative Threshold Events
F5=Cumulative Program NAND Pages
F6=Total Host Sector Writes
F7=Host Program Page Count
F8=Background Program Page Count

[SmartMicronMU02] ;Updated 6.6.0
; RAIN = Redundant Array of Independent NAND
01=Raw Read Error Rate
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
0D=Soft Error Rate
0E=Device Capacity (NAND)
0F=User Capacity
10=Spare Blocks Available
11=Remaining Spare Blocks
64=Total Erase Count
AA=Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Block-Erase Count
AE=Unexpected Power Loss Count
B4=Unused Reserve NAND Blocks
B7=SATA Interface Downshift
B8=Error Correction Count
BB=Reported Uncorrectable Errors
BC=Command Timeout Count
BD=Factory Bad Block Count
C2=Temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Smart Off-line Scan Uncorrectable Error Count
C7=Ultra DMA CRC Error Rate
CA=Percent Lifetime Used
CE=Write Error Rate
D2=Successful RAIN Recovery Count
EA=Total Bytes Read
F3=ECC Bits Corrected
F4=ECC Cumulative Threshold Events
F5=Cumulative Program NAND Pages
F6=Total Host Sector Writes
F7=Host Program Page Count
F8=Background Program Page Count

; Updated 6.6.0
A0=Uncorrectable Sector Count
A1=Valid Spare Blocks
A3=Initial Invalid Blocks
94=Total SLC Erase Count
95=Maximum SLC Erase Count
96=Minimum SLC Erase Count
97=Average SLC Erase Count
A4=Total TLC Erase Count
A5=Maximum TLC Erase Count
A6=Minimum TLC Erase Count
A7=Average TLC Erase Count
A9=Percentage Lifetime Remaining
B5=Program Fail Count
B6=Erase Fail Count
C0=Power-off Retract Count
E8=Available Reserved Space
F1=Total LBA Write
F2=Total LBA Read
F5=Total TLC Write Count
F6=Total SLC Write Count
F7=RAID Recovery Count

[SmartOcz] ;Added (4.5)
01=Raw Read Error Rate
03=Spin Up Time
04=Start Stop Count
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
E8=Total Count of Write Sectors
E9=Remaining Life

; Added 6.6.0
64=Total Blocks Erased
A7=SSD Protect Mode
A8=SATA PHY Error Count
A9=Bad Block Count
AD=Erase Count
B8=Factory Bad Block Count
C0=Unexpected Power Loss Count
CA=Total Number of Corrected Bits
CD=Max Rated PE Counts
CE=Minimum Erase Counts
CF=Maximum Erase Counts
D3=SATA Uncorrectable Error Count
D4=NAND Page Reads During Retry
D5=Simple Read Retry Attempts
D6=Adaptive Read Retry Attempts
DD=Internal Data Path Uncorrectable Errors
DE=RAID Recovery Count
E6=Power Loss Protection
FB=NAND Read Count

;Updated 6.7.0
F1=Total Host Writes
F2=Total Host Reads

[SmartPlextor] ;Added (5.1.0)/Updated (5.4.0)
01=Read Error Rate
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
AA=Grown Bad Blocks
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Program/Erase Count
AE=Unexpected Power Loss Count
AF=Program Fail Count (Worst Case)
B0=Erase Fail Count (Worst Case)
B1=Wear Leveling Count
B2=Used Reserved Block Count (Worst Case)
B3=Used Reserved Block Count
B4=UnUsed Reserved Block Count (Total)
B5=Program Fail Count
B6=Erase Fail Count
B7=SATA Interface Down Shift
B8=End-to-End Data Errors Corrected
BB=Uncorrectable Error Count
BC=Command Time out
C0=Unsafe Shutdown Count
C3=ECC rate
C4=Reallocation Event Count
C6=Uncorrectable Sector Count
C7=Ultra CRC Error Count
E8=Available Reserved Space
E9=NAND GB written
F1=Total Host Writes
F2=Total Host Reads

[SmartSanDisk] ;Added (5.2.0)
05=Retired Block Count
09=Power-On Hours
0C=Power Cycle Count
AA=Reserve Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
BB=Reported Uncorrectable Errors
E8=Remaining Life
F1=Total Host Writes
F2=Total Host Reads

[SmartOczVector] ;Added (5.3.0)
05=Accumulated Runtime Bad Blocks
09=Power-On Hours Count
0C=Power Cycle Count
AB=Available Over-Provisioned Block Count
AE=Power Cycle Count (Unplanned)
BB=Total Uncorrectable NAND Reads
C3=Total Programming Failures
C4=Total Erase Failures
C5=Total Read Failures (Uncorrectable)
C6=Host Reads
C7=Host Writes
D0=Average Erase Count
D2=SATA CRC Error Count
E9=Remaining Life
F9=Total NAND Programming Count

;Updated 5.5.0
F1=Total Host Writes
F2=Total Host Reads

;Updated 6.6.0
64=Total Blocks Erased
B8=Factory Bad Block Count Total
CA=Total Number Of Read Bits Corrected
CD=Max Rated PE Count
CE=Min Erase Count
CF=Max Erase Count
D4=Total Count NAND Pages Reads Requiring Read Retry
D5=Total Count of Simple Read Retry Attempts
D6=Total Count of Adaptive Read Retry Attempts
DD=Internal Data Path Protection Uncorrectable Errors
DE=RAID Recovery Count
E0=In Warranty
E1=DAS Polarity
E2=Partial Pfail
E6=Write Throttling Activation Flag
F9=Total NAND Programming Count (pages)
FB=Total NAND Read Count

[SmartCorsair] ;Added 6.2.0
01=Raw Read Error Rate
05=Retired Block Count
09=Power On Hours
0C=Power Cycle Count
AA=Reserve Block Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
B5=Program Fail Count
BB=Reported Uncorrectable Errors
C2=Temperature
C4=Reallocation Event Count
E7=SSD Life Left
F1=Lifetime GB Written
F2=Lifetime GB Read

[SmartToshiba] ;Added 6.2.0
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
04=Start/Stop Count
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0B=Recalibration Retries
0C=Power Cycle Count
A7=SSD Protect Mode
A8=SATA PHY Error Count
A9=Total Bad Block Count
AD=Erase Count
C0=Unexpected Power Loss Count
C2=Temperature
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Uncorrectable Sector Count
F1=Total Host Writes
F2=Total Host Reads

[SmartSanDiskGb] ;Added 6.2.0
05=Reallocated Block Count
09=Power On Hours
0C=Power Cycle Count
A6=Min W/E Cycle
A7=Max Bad Block/Die
A8=Maximum Erase Cycle
A9=Total Bad Block
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Erase Cycle
AE=Unexpected Power Loss Count
BB=Reported Uncorrectable Errors
C2=Temperature
D4=SATA PHY Error
E6=Percentage Total P/E Count
E8=Spare Block Remaining
E9=Total GB Written To NAND
F1=Total GB Written
F2=Total GB Read

[SmartKingston] ;Added 6.6.0
01=Read Error Rate
02=Throughput Performance
03=Spin Up Time
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0C=Power Cycle Count
A8=SATA PHY Error Count
AA=Bad Block Count
AD=Erase count
AF=Bad Cluster Table Count
BB=Uncorrectable Errors
C0=Unsafe Shutdown Count
C2=Temperature
C4=Later Bad Block Count
C5=Current Pending Sector Count
C7=CRC Error Count
DA=CRC Error Count
E7=SSD Life Left
E9=Lifetime Writes to Flash
F0=Write Head
F1=Host Writes
F2=Host Reads
F4=Average Erase Count
F5=Max Erase Count
F6=Total Erase Count

[SmartNVMe] ;Added 6.7.0
01=Critical Warning
02=Composite Temperature
03=Available Spare
04=Available Spare Threshold
05=Percentage Used
06=Data Units Read
07=Data Units Written
08=Host Read Commands
09=Host Write Commands
0A=Controller Busy Time
0B=Power Cycles
0C=Power On Hours
0D=Unsafe Shutdowns
0E=Media and Data Integrity Errors
0F=Number of Error Information Log Entries

[SmartRealtek] ;Added by Realtek
01=Raw data error rate
05=Reallocated sector count
09=Power on hour count
0C=Power cycle count
A1=GDN
A2=Total erase count
A3=Max PE cycle
A4=Average erase count
A5=Initial bad block count
A6=Total bad block count
A7=SSD protect mode
A8=SATA Phy error count
A9=Health
AB=Program fail count
AC=Erase fail count
AE=Unexpected power loss count
AF=ECC fail count
B5=Unaligned access count
BB=Reported uncorrectable error
C2=Enclosure temperature
C3=Cumulative corrected ecc
C4=Reallocation event count
C7=Ultra DMA CRC error count
CE=Min. erase count
CF=Max erase count
E7=Lifetime left
E8=Available reserved space
F1=Write life time
F2=Read life time
F9=Total GB written to NAND (TLC)
FA=Total GB written to NAND (SLC)

[SmartSKhynix] ; Updated 8.8.0
01=Read Error Rate
05=Re-Assigned Sector Count
09=Power-On Hours
0C=Power Cycle Count
64=Total Erase Count
A8=Min. Erase Count
A9=Max. Erase Count
AA=Reserve Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
AF=Program Fail Count(Worst Case)
B0=Erase Fail Count(Worst Case)
B1=Wear Leveling Count
B2=Used Reseved Block Count(Worst Case)
B3=Used Reseved Block Count(SSD Total)
B4=UnUsed Reseved Block Count(SSD Total)
B5=Program Fail Count(SSD Total)
B6=Erase Fail Count(SSD Total)
B7=SATA Downshift Count
B8=End-to-End Error Detection Count
BB=Uncorrectable Error Count
BC=Command Timeout Count
BF=Op Shock Event Count
C2=Temperature
C3=ECC Rate
C4=Reallocation Event Count
C6=Uncorrectable Sector Count
C7=CRC Error Count
C9=Uncorrectable Soft Read Error Rate
CC=Soft ECC Correction Rate
D4=Phy Error Count
E7=SSD Life Left
E9=SSD Life Left
EA=NAND Written
F1=Total LBA Written
F2=Total LBA Read
FA=Total Number of NAND Read Retries

[SmartKioxia]
09=Power-On Hours Count
0C=Device Power Cycle Count
A7=SSD Protect Mode
A8=SATA PHY Error Count
A9=Bad Block Count
AD=Erase Count (User Data)
C0=Unexpected Power Loss Count
C2=Temperature
F1=Host Writes

[SmartWdc]
01=Read Error Rate
05=Reassigned Block Count
09=Power On Hours
0C=Power Cycle Count
A5=Block Erase Count (SLC)
A6=Minimum P/E Cycles
A7=Maximum Bad Blocks per die
A8=Maximum P/E Cycles
A9=Total Bad Block
AA=Grown Bad Blocks
AB=Program Fail Count
AC=Erase Fail Count
AD=Average P/E Cycles
AE=Unexpected Power Loss Count
B8=End-to-End Error Detection/Correction Count
BB=Reported Uncorrectable Errors
BC=Command Timeout Count
C2=Temperature
C7=CRC Error Count
D4=SATA PHY Error
E6=Media Wearout Indicator
E8=Available Reserve Space
E9=NAND GB Written
EA=NAND GB Written (SLC)
EE=Media Wearout Indicator (Cycles Remaining)
F1=Total GB Written
F2=Total GB Read
F4=Temperature Throttle Status
F9=NAND GB Written

[SmartKingstonSuv]
01=Read Error Rate
05=Reallocated Sector Count
09=Power On Hours
0C=Power Cycle Count
AA=Used Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Off Count
AF=Program Fail Count Worst Die
B0=Erase Fail Count Worst Die
B1=Wear Leveling Count
B2=Used Reserved Block Count worst Die
B4=Unused Reserved Block Count (SSD Total)
BB=Reported Uncorrectable Errors
C2=Temperature
C3=On-the-Fly ECC Error Count
C4=Reallocation Event Count
C5=Pending Sector Count
C7=UDMA CRC Error Count
C9=Uncorrectable Read Error Rate
CC=Soft ECC Correction Rate
E7=SSD Life Left
EA=Lifetime Nand Writes
F1=Lifetime Host Writes
F2=Lifetime Host Reads
FA=Total Number of NAND Read Retries

[SmartKingstonKC600]
01=Read Error Rate
05=Re-Allocated NAND Block Count
09=Power-On Hours
0C=Power Cycle Count
94=Reserved
95=Reserved
96=Reserved
97=SLC Average Erase Count
9F=DRAM 1 bit Error Count
A0=Reported UECC (UnCorrectable) Errors
A1=Available Reserved Space
A4=Reserved
A5=Reserved
A6=Reserved
A7=Average Erase Count
A8=Reserved
A9=Percentage Of Rated Lifetime Remaining
B1=Reserved
B5=Program Fail Count
B6=Erase Fail Count
C0=Unexpected Power Loss Count
C2=Device Temperature
C3=Hardware ECC Recovered
C4=Reallocation Event Count
C7=UDMA CRC Error Count
E7=Percentage of Rated Lifetime Remaining
E8=Unused Reserved Block Count
F1=Total LBAs Written
F2=Total LBAs Read
F5=Total Media Writes

[SmartKingstonDC500]
01=Host UNC Error Count
09=Power on Hours
0C=Power On / Off Cycle
A7=Protect mode
A8=SATA PHY Error Count
A9=Bad Block Rate
AA=Bad Block Information
AC=Erase Failure Count
AD=Erase Count
B5=Program Fail Count
B6=Erase Failure Count
BB=Host UNC Error Count
C0=Unexpected Power Loss Count
C2=Temperature
C4=Total Later Bad Block Count
C7=CRC Error Count
CF=Thermal Throttling Count
DA=CRC Error Count
E7=SSD Life Remaining
E8=Read Fail Count
E9=NAND Write
F1=Host Write
F2=Host Read
F4=Avg Erase Count
F5=Max Erase Count
F6=Total Erase Count

[SmartKingstonSA400]
01=Uncorrectable Errors
09=Power On Hours
0C=Power Cycles
94=Vendor Unique
95=Vendor Unique
A7=Vendor Unique
A8=SATA PHY Error Count
A9=Vendor Unique
AA=Bad Block Count
AC=Vendor Unique
AD=Erase Count
B5=Vendor Unique
B6=Vendor Unique
BB=Uncorrectable ECC Errors
C2=Temperature
C4=Reallocation Events
C7=SATA CRC Error
DA=CRC Error Count
E7=SSD Wear Indicator
E9=Lifetime Nand Writes
F1=Lifetime Writes from Host
F2=Lifetime Read from Host
F4=Average Erase Count
F5=Max Erase Count
F6=Total Erase Count

[SmartSsstc]
01=Raw Read Error Rate
05=Reallocated Block Count
09=Power On Hours
0C=Power Cycle Count
AA=Available Reserved Space
AB=Program Fail Count(Total)
AC=Erase Fail Count(Total)
AD=Average Program/Erase Count
AE=Unexpected Power Loss Count
AF=Program Fail count (Worst case)
B0=Erase Fail Count (Worst case)
B1=Wear Leveling Count
B2=Used Reserved Block Count (Worst case)
B3=Used Reserved Block Count (Total)
B4=Unused Reserved Block Count (Total)
B7=SATA Interface Down shift
B8=End-to-End Data Errors Count
BB=Uncorrectable Error Count
BC=Command Time out
C2=Drive Temperature
C3=ECC rate
C6=OffLine Uncorrectable Error Count
C7=SATA CRC Error Count
E5=Power Loss Protection Failure
E7=Percentage Lifetime Remaining
E8=Available Reserved Space 
E9=NAND GB Written
F1=Total Host Write
F2=Total Host Read 
F3=NAND GB Written

[SmartIntelDc]
01=Raw Read Error Count
05=Reallocated Flash Block Count
09=Power-On Hours Count
0C=Power Cycle Count
0E=Device Capacity
0F=User Capacity
10=Spare Blocks Available
11=Remaining Spare Available
AC=Total Block Erase Failure
AD=Per Block Max Erase Count
AE=Unexpected Power Loss Count
AF=Average Erase Count
B0=Power Loss Protection Error
B5=Total Block Program Failure
B8=End-to-End Error Detection Count
BB=Uncorrectable Error Count
C2=Temperature
C5=Pending Sector Count
C6=Offline Uncorrectable Error Count
C7=CRC Error Count
CA=Percentage of Drive Life Used
E2=Timed Workload - Media Wear
E3=Timed Workload - Host Read/Write Ratio
E4=Timed Workload Timer
EA=Total Host Bytes Read
EB=Total Host Bytes/Sectors Written
F1=Total Nand Bytes/Sectors Written

[SmartApacer]
09=Power on Hours
0C=Power Cycle Count
A3=Maximum Erase Count
A4=Average Erase Count
A6=Total Later Bad Block Count
A7=SSD Protect Mode
A8=SATA PHY Error Count
AB=Program Fail Count
AC=Erase Fail Count
AF=Bad Cluster Table Count
C0=Unexpected Power Loss Count
C2=Temperature
E7=Lifetime Left
F1=Total Sectors Write

[SmartSiliconMotion]
01=Read Error Rate
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
94=SLC Total Erase Count
95=SLC Maximum Erase Count
96=SLC Minimum Erase Count
97=SLC Average Erase Count
9F=DRAM 1 bit Error Count
A0=Uncorrectable sectors count when read/write
A1=Number of Valid Spare Blocks
A2=Number of Cache Data Block
A3=Number of Initial Invalid Blocks
A4=Total Erase Count
A5=Maximum Erase Count
A6=Minimum Erase Count
A7=Average Erase Count
A8=Max Erase Count of Spec
A9=Remain Life
AF=Program fail count in worst die
B0=Erase fail count in worst die
B1=Total Wear Level Count
B2=Runtime Invalid Block Count
B5=Total Program Fail Count
B6=Total Erase Fail Count
BB=Uncorrectable Error Count
C0=Power-Off Retract Count
C2=Temperature
C3=Hardware ECC Recovered
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Uncorrectable Error Count Off-line
C7=Ultra DMA CRC Error Count
E8=Available Reserved Space
F1=Total LBA Written
F2=Total LBA Read
F5=Flash Write Sector Count

[SmartJMicron66x]
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0C=Power Cycle Count
A8=SATA PHY Error Count
AA=Bad Block Count
AD=Erase Count
AF=Bad Cluster Table Count
B4=Spare Block Count
C0=Unexpected Power Loss Count
C2=Temperature
C5=Current Pending Sector Count
E7=Drive Life
E9=Write Sector Count (NAND)
F0=Write Head
F1=Total LBA Written
F2=Total LBA Read

[SmartPhison]
01=Read Error Rate
09=Power on Hours
0C=Power Cycle Count
A8=SATA PHY Error Count
AA=Bad Block Count
AD=Erase Count
C0=Unexpected Power Loss Count
C2=Temperature
DA=Number of CRC Error
E7=SSD Life Left
F1=Host Writes

[SmartSeagate]
01=Read Error Rate
05=Retired Sectors Count
09=Power On Hours
0C=Power Cycle Count
10=Spare Blocks Available
11=Remaining Spare Blocks
A8=SATA PHY Error Count
AA=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B5=Program Fail Count
B6=Erase Fail Count
C0=Unexpected Power loss Count
C2=Temperature
C9=Soft Error Rate
CC=Soft ECC Correction Rate
DA=CRC Error Count
E7=SSD Life Left
E8=Read Failure Block Count
E9=NAND GiB Written
EA=Lifetime Writes To Flash
EB=NAND sectors Written
F1=Lifetime Writes From Host
F2=Lifetime Reads From Host
FA=Lifetime NAND Read Retries

[SmartSeagateIronWolf]
01=Raw Read Error Rate
05=Reallocated Sector Count
09=Power On Hours
0C=Power Cycle Count
64=Flash Gigabytes Erased
66=Lifetime PS4 Entry Count
67=Lifetime PS3 Entry Count
AA=Grown Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Program/Erase Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B7=SATA/PCIe Interface Downshift Count
BB=Uncorrectable ECC Count
C2=Temperature
C3=RAISE ECC Correctable Count
C6=Uncorrectable Read Error Count
C7=SATA R-Error (CRC) Error Count
E6=Drive Life Protection Status
E7=SSD Life Left
E8=Available Reserved Space
E9=Lifetime Writes to Flash
F1=Lifetime Writes From Host
F2=Lifetime Reads From Host
F3=Free Space

[SmartMarvell] ; Added 8.8.3
05=Number of New Bad Block
09=Power On Hours
0C=Power Cycle Count
A4=Total Erase Count
A5=Maximum Erase Count
A6=Minimum Erase Count
A7=Average Erase Count
C0=Power off Retract Count
C2=Temperature
C7=SATA CRC Error Count
F1=Total Written
F2=Total Read

[SmartMaxiotek] ; Added 8.8.6
05=Reallocated Sector Count
09=Power-On Hours
0C=Drive Power Cycle Count
A7=SSD Protect Mode
A8=PHY Error Count
A9=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AF=Bad Cluster Table Count
B1=Read Retry Count
B4=Spare Block Count Left
BB=Reported UNC Errors
C0=Unexpected Power Loss Count
C2=Temperature
C4=Reallocated Event Count
C7=UDMA CRC Error Count
CE=Minimum Erase Count
CF=Maximum Erase Count
D0=Average Erase Count
D1=Minimum Erase Count of SLC block
D2=Maximum Erase Count of SLC block
D3=Average Erase Count of SLC block
E7=SSD Life Left
E9=Write Counts Sectors to Nand
EA=Read Counts Sectors from Nand
F1=Write Sector Count
F2=Read Sector Count
F5=Bit Error Count

[SmartSeagateBarraCuda] ; Added 8.9.0
01=UECC Error Count
05=Retired Sectors Count
09=Power On Hours
0C=Power Cycle Count
10=Spare Blocks Available
11=Remaining Spare Blocks
A8=SATA PHY Error Count
AA=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B5=Program Fail Count
B6=Erase Fail Count
C0=Unexpected Power loss Count
C2=Temperature
C9=Soft Error Rate
CC=Soft ECC Correction Rate
DA=CRC Error Count
E7=SSD Life Left
E8=Read Failure Block Count
E9=NAND GiB Written
EA=Lifetime Writes To Flash
EB=NAND sectors Written
F1=Lifetime Writes From Host
F2=Lifetime Reads From Host
FA=Lifetime NAND Read Retries

[SmartYmtc] ; Added 8.10.0
05=New Bad Block Count
09=Power-On Hours Count
0C=Power Cycle Count
AA=Max Bad Block Count
A8=SATA PHY Error Count
A9=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AF=Bad Cluster Count
B7=SATA Interface Downshift
B8=End to End Error Detection/Correction Count
BB=Uncorrectable Error Count
BE=Temperature
C0=Unexpected Power Loss Count
C4=Re-allocated Event Count
C7=CRC Error Count
CE=Minimum Erase Count
CF=Maximum Erase Count
D0=Average Erase Count
D1=SLC Minimum Erase Count
D2=SLC Maximum Erase Count
D3=SLC Average Erase Count
E7=SSD Life Left
E9=Write sector count to NAND
EA=Read sector count to NAND
F1=Total LBA written
F2=Total LBA Read
F3=NAND Temperature
F5=Bit Error Count

[SmartScy] ;Added 8.12.8
01=Raw Read Error Rate
05=Reallocated Sector Count
07=Seek Error Rate
09=Power-On Hours
0C=Drive Power Cycle Count
A7=Average Erase Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
B1=Read Retry Count
B4=Spare Block Count Left
B7=Runtime Bad Block
BB=Reported UNC Errors
C0=Unexpected Power Loss Count
C2=Controlled Temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocated Event Count
C5=Current Pending Sector
C7=UDMA CRC Error Count
E7=SSD Life Left
F1=Total LBAs Written
F2=Total LBAs Read
F5=Total Nand Flash Written

[SmartRecadata] ;Added 8.14.0
07=Seek Error Rate
09=Power-On Hours
0C=Drive Power Cycle Count
A7=Average erase count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
B1=Read Retry Count
B4=Spare Block Count Left
B7=Runtime Bad Block
BB=Reported UNC Errors
C0=Unexpected Power Loss Count
C2=Controlled temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocated Event Count
C5=Current Pending Sector
C7=UDMA CRC Error Count
E7=SSD Life Left
F1=Total LBAs written
F2=Total LBAs read
F5=Total Nand Flash Written
